|  |
| --- |
| **CE****EC Declaration of Performance** |
| Lime Green Products Ltd, Coates Kilns, Stretton Road, Much Wenlock, Shropshire, TF13 6DG13 |
| **EN 998–1:2010****General purpose (GP) rendering mortar for external use****Reaction to fire:** Class A 1**Adhesion:** 0.9N/mm2 FP: b**Capillary Water absorption:** W0**Water vapour Permeability coefficient.** ≤15**Thermal conductivity λ10,dry [W/mK] *P=50%*** 0.67 ***P= 90%*** 0.76 **Durability:** (against freeze/thaw)**:** evaluation based on provisions valid in the intended place of use of the mortar |

**Lime Green Natural Stipple**

**Date** 28/8/13

**Signed**

J Ayres – Director